|  |  |  |
| --- | --- | --- |
|  | **VEHICLE ENTRY PERMIT** | Permit reg. No: |
| Reg. date: |
| Validity date: from \_\_\_\_\_\_\_\_\_ to \_\_\_\_\_\_\_\_\_ Time: from \_\_\_\_ hr. to \_\_\_\_ hr.  Organizational unit \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_  Company-owner of the vehicle \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_  Make and plate number of the vehicle \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_  Purpose of entry \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_  \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_  Mandatory requirement to use gas analyzer: **🖵** Yes **🖵** No | | |
| Agree and accept the safety requirements:  \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_  (Driver’s full name & signature) | | |
| Entry to the hazard area allowed:  \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_  (Job title, full name and signature of permit issuer) | | |
| **SAFETY REGULATIONS**  **Requirements for Vehicles**   * Affix the permit to the vehicle windscreen and keep it there for the entire duration of the vehicle presence in the hazard area. * Keep the vehicle emergency flashers on. * Speed limit of 20 km/h must be observed. * Park the vehicle reverse (facing the exit). * Leave the hazard area after completion of works.   **Emergency procedures**   * In case of any leaks of dangerous substances, activation of emergency alarm or gas analyzer, immediately discontinue the work, switch the vehicle engine off, leave the vehicle unlocked, and notify the relevant process unit staff. * In case of a fire, accident, or emergency during the vehicle operation, the permit ceases to be effective and shall be handed over to the respective investigation committee. | | |