Public Company ORLEN Lietuva Occupational Health and Safety Procedure BDS-10

Use of Work Equipment in Potentially Explosive Atmospheres Attachment 1

|  |  |  |
| --- | --- | --- |
| **OL_logo_pilkasbaltame** | **Permit to Use Work Equipment in Potentially Explosive Atmospheres (permit form)** | **Reg. No. \_\_\_\_\_\_\_\_\_\_\_**  **Reg. date \_\_\_\_\_\_\_** |
| Validity date from \_\_\_\_\_\_\_\_ to \_\_\_\_\_\_\_\_ Time from \_\_\_\_\_\_ hr. to \_\_\_\_\_\_ hr.  Organizational unit \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Place of Use \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_  Org. unit, contractor using the equipment \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_  Work equipment \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_  Purpose \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_  \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ | | |
| Agree and accept the safety requirements:  \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_  (User's job title, full name and signature) | | |
| I hereby allow to use the equipment  \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_  (Job title, full name and signature of person authorized to issue a permit) | | |

The reverse side of permit

|  |
| --- |
| **SAFETY REQUIREMENTS**  **VEHICLE REQUIREMENTS**  ● Attach the permit to the vehicle windscreen and keep it there for the duration of vehicle presence in the unit territory.  ● Keep the vehicle emergency flashers on.  ● Driving speed shall not exceed 20 km/h.  ● Park the vehicle reverse (facing the exit).  **●** Leave the unit territory after completion of works.  **Emergency procedures**  ● In case of leak of dangerous substances, operation of emergency alarm or gas analyzer, immediately stop the works, shut down the vehicle engine or equipment, and notify the process staff.  ● In case of fire, accident, emergency during the use of equipment, permit becomes invalid and must be handed over to the respective investigation committee. |