Public Company ORLEN Lietuva Occupational Health and Safety Procedure BDS-10

Use of Work Equipment in Potentially Explosive Atmospheres Attachment 1

|  |  |  |
| --- | --- | --- |
| **OL_logo_pilkasbaltame** | **Permit to Use Work Equipment in Potentially Explosive Atmospheres (permit form)** | **Reg. No. \_\_\_\_\_\_\_\_\_\_\_****Reg. date \_\_\_\_\_\_\_** |
| Validity date from \_\_\_\_\_\_\_\_ to \_\_\_\_\_\_\_\_ Time from \_\_\_\_\_\_ hr. to \_\_\_\_\_\_ hr.Organizational unit \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Place of Use \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Org. unit, contractor using the equipment \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Work equipment \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Purpose \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ |
| Agree and accept the safety requirements: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_(User's job title, full name and signature) |
| I hereby allow to use the equipment \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_(Job title, full name and signature of person authorized to issue a permit) |

The reverse side of permit

|  |
| --- |
| **SAFETY REQUIREMENTS****VEHICLE REQUIREMENTS**● Attach the permit to the vehicle windscreen and keep it there for the duration of vehicle presence in the unit territory.● Keep the vehicle emergency flashers on. ● Driving speed shall not exceed 20 km/h.● Park the vehicle reverse (facing the exit). **●** Leave the unit territory after completion of works. **Emergency procedures**● In case of leak of dangerous substances, operation of emergency alarm or gas analyzer, immediately stop the works, shut down the vehicle engine or equipment, and notify the process staff.● In case of fire, accident, emergency during the use of equipment, permit becomes invalid and must be handed over to the respective investigation committee. |